## Maintaining Wi-Fi Towers

Step | Action
1. | Begin by navigating to the Maintain Wi-Fi Towers page. Click the Maintain Wi-Fi Towers link.
2. | Use the View Wi-Fi Towers page see the location of your Wi-Fi towers.
3. | Use the Pan tool to navigate from left to right and top to bottom of the map.
4. | Use the Zoom in and Zoom out tool, to get the desired view area.
5. | Pointing to a Wi-Fi tower opens a dialog box with the tower name and latitude and longitude information.
6. | The Distance button provides the distance between two or more towers. Click the Distance button.
7. | Select the tower you want as the start point to measure the distance. Click the Wi-Fi Tower object.
8. | Select another tower. Click the Wi-Fi Tower object.
9. | The distance between the two towers populates in the bottom left corner of the map.
10. | The Area button gives you the area between towers. Click the Area button.
11. | Select the tower you want as the start point to measure the area. Click the Wi-Fi Tower object.
12. | Select another tower. Click the Wi-Fi Tower object.
13. | Select another tower. Click the Wi-Fi Tower object.
14. | The area between the towers populates at the bottom left corner of the map.
15. | The Information button provides the latitude and longitude information of the selected area. Click the Information button.
16. | The latitude and longitude information is shown at the bottom left corner of the map.
17. | Next, proceed to the Maintain Wi-Fi Towers page to add and remove Wi-Fi towers. Click the Maintain Wi-Fi Towers button.
18. | Click the View menu.
19. | Use the Columns option to manage columns. Use the Detach option to view the table separately. Use the Reorder Columns... option to rearrange columns.
20. | First, add a Wi-Fi tower. Click the Add Wi-Fi button.
21. | A new row with an automatically populated Tower ID appears.
22. | Enter the latitude of the Wi-Fi tower location. Click in the Latitude field.
23. | Enter the desired information into the Latitude field. Enter a valid value e.g. "37.748".
24. | Enter the longitude of the Wi-Fi tower location. Click in the Longitude field.
25. | Enter the desired information into the Longitude field. Enter a valid value e.g. "-122.478".
26. | Use the Range (meters) field to specify a range within which devices can be considered for offloading. Click in the Range (meters) field.
27. | Enter the desired information into the Range (meters) field. Enter a valid value e.g. "500".
28. | Use the Description field to add an optional description. Click in the Description field.
29. | Enter the desired information into the Description field. Enter a valid value e.g. "Daly City".
30. | Save the Wi-Fi tower. Click the Save button.
31. | The Wi-Fi tower is now pinned to the corresponding location on the map.
32. | Next, edit a Wi-Fi tower. Click the Maintain Wi-Fi Towers button.
33. | Edit the range for the Wi-Fi tower MDO_WIFI000018. Click in the Range (meters) field.
34. | Enter the desired information into the Range (meters) field. Enter a valid value e.g. "300".
35. | Click the Save button.
36. | The tower range is now modified.
37. | Next, remove a Wi-Fi tower. Select the Wi-Fi tower you want to delete. Click an entry in the row.
38. | Click the Remove Wi-Fi button.
39. | Confirm that you want to delete the Wi-Fi tower. Click the Yes button.
40. | Click the Save button.
41. | The Wi-Fi tower MDO_WIFI000018 is now removed.
42. | You have completed the Maintaining Wi-Fi Towers topic. End of Procedure.